**Machine Inspection**

**Site:** Broadlea Mine - Golding

**Machine Model:** Komatsu 730E-7

**Serial Number:**  A30270 - 1807

Truck is in overall good condition, currently does not run as a couple parts have been removed but Goldings will replace to get it going again

* Cab in decent condition
* All cylinders and struts are free of oil leaks
* Mesabi radiator
* All panels, platforms, walkways are in good condition
* No major visible oil leaks coming from truck
* Alternator model: 5GTA22M2 SN: EE03110653
* LH Wheel Motor Model: 5GE788HS10 SN: 95100818
* RH Wheel Motor Model: 5GE788HS10 SN: W96046103
* Rear Struts are rod down type
* Slight leak from fuel tank sight glass

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Position** | **Size** | **Brand** | **Serial** | **Type** | **Tread** | **Condition** |
| 1 | 40.00R57 | Bridgestone | SOR 004 575 | 3A | 95/96 | Excellent |
| 2 | 40.00R57 | Bridgestone | SOR 004 579 | 3A | 96/96 | Excellent |
| 3 | 40.00R57 | Michelin | JLG 1025 T1A | XDR3 MC4 | 78/75 | Good |
| 4 | 40.00R57 | Michelin | JLG 1044 T2A | XDR3 MC4 | 77/74 | Good  |
| 5 | 40.00R57 | Michelin | CVZ 0234 E4A | XDR3 MC4 | 86/85 | Good |
| 6 | 40.00R57 | Michelin | CVZ 0221 E7A | XDR3 MC4 | 86/89 | Good |

All Tyres are in good condition with no visible damage.

Over all truck is in good condition with no visible faults, currently not running due to a few small missing parts, but Golding will get it operational again for demobbing.